**General specifications and requirements for supplying brake pads**

1. The brake pads must have the European quality test homologation (ratification ) according to the European regulation such as ECE no90.
2. The brake pads must not whistle (no noise) and must not have any smell.
3. The brake pads must have long durability and performance.
4. No dust.
5. Asbestos free.
6. Each set must have installation instructions.
7. Importer identification card and goods description must be printed/labeled on the carton box of each brake pad (An example will be provided).
8. Guarantee of the brake pads is required.
9. The break pads should include all the complete accessories such as wires, screws, …).
10. Printing on the brake pad the company name, Test No., and reference No.
11. Each piece should be packaged with a sealed nylon bag with the company name printed on the nylon bag in addition to the outside carton box .
12. The materials used must be as the original materials used for the brake pads.
13. As requirement for shipping products to Israel, a declaration about the products and quality must be signed by the manufacturer and signed by the Chamber of Commerce or Notary public (a copy is attached ).